; Copyright (c) 1995-2000 Microsoft Corporation.  All rights reserved.
MODULES
;  Name            Path                                           Memory Type
;  --------------  ---------------------------------------------  -----------
IF IMGTINY !
IF IMGNODRIVERS !

IF IMGNOCEDDK !
   ceddk.dll       $(_FLATRELEASEDIR)\pc_ddk.dll                NK  SH
ENDIF

; USB drivers
IF ODO_NOUSB !

IF IMGUSB
IF CEPC_UHCI
   uhci.dll       $(_FLATRELEASEDIR)\uhci.dll                   NK  SH
ENDIF
IF CEPC_OHCI
   ohci.dll       $(_FLATRELEASEDIR)\ohci.dll                   NK  SH
ENDIF
   usbd.dll       $(_FLATRELEASEDIR)\usbd.dll                   NK  SH
   usbhid.dll     $(_FLATRELEASEDIR)\usbhid.dll                 NK  SH
ENDIF

ENDIF

; CEPC Serial Mouse Driver
IF CEPC_SERMOUSE
   sermouse.dll   $(_FLATRELEASEDIR)\sermouse.dll               NK  SH
ENDIF

;
; MGDI Display driver
; The default display driver is the S3Trio64 display
; To use the 8BPP generic VGA set the environment variable
; CEPC_DDI_VGA8BPP to 1.  To use the CT driver, set
; CEPC_DDI_CT655X to 1. To use the accelerated S3ViRGE driver
; set CEPC_DDI_S3VIRGE to 1.

IF ODO_NODISPLAY !

IF CEPC_DDI_VGA8BPP
   ddi.dll         $(_FLATRELEASEDIR)\ddi_vga8.dll              NK  SH
ENDIF
IF CEPC_DDI_CT655X
   ddi.dll         $(_FLATRELEASEDIR)\ddi_ct.dll                NK  SH
ENDIF
IF CEPC_DDI_S3VIRGE
   ddi.dll         $(_FLATRELEASEDIR)\ddi_s3v.dll               NK  SH
ENDIF
IF CEPC_DDI_S3TRIO64
   ddi.dll         $(_FLATRELEASEDIR)\ddi_s364.dll              NK  SH
ENDIF
IF CEPC_DDI_FLAT
   ddi.dll         $(_FLATRELEASEDIR)\ddi_flat.dll              NK  SH
ENDIF
IF CEPC_DDI_ATI
   ddi.dll         $(_FLATRELEASEDIR)\ddi_ati.dll               NK  SH
ENDIF
IF CEPC_DDI_FLAT !
IF CEPC_DDI_S3VIRGE !
IF CEPC_DDI_CT655X !
IF CEPC_DDI_VGA8BPP !
IF CEPC_DDI_S3TRIO64 !
IF CEPC_DDI_ATI !
   ddi.dll         $(_FLATRELEASEDIR)\ddi_flat.dll              NK  SH
ENDIF
ENDIF
ENDIF
ENDIF
ENDIF
ENDIF
ENDIF
ENDIF

IF ODO_NOKEYBD !

IF COUNTRY=JAPAN !
    kbdmouse.dll     $(_FLATRELEASEDIR)\KbdMsEngUs1.dll               NK  SH
ENDIF
IF COUNTRY=JAPAN
    kbdmouse.dll     $(_FLATRELEASEDIR)\KbdMsJpn2.dll               NK  SH
ENDIF

ENDIF

IF ODO_NOAUDIO !
   wavedev.dll     $(_FLATRELEASEDIR)\wavedev.dll                 NK  SH
ENDIF

IF ODO_NOSERIAL !

IF NEW_SERIAL_MDD
; And the com16550 driver supports any number of 16550 ports.
   com16550.dll    $(_FLATRELEASEDIR)\com16550.dll                NK  SH
; Note - The serial driver is now split into a PCMCIA modem driver and a
; builtin 16550 driver.  But all the PNP entries say to use serial.dll
; for PCMCIA modems, So for now lets just call it serial.dll in the image
   serial.dll      $(_FLATRELEASEDIR)\com_card.dll                NK  SH
ENDIF
IF NEW_SERIAL_MDD !
; Old serial driver is monolithic DLL for builtin and modem
   serial.dll      $(_FLATRELEASEDIR)\serial.dll                  NK  SH
ENDIF
IF IMGSL11
   sl11_ser.dll    $(_FLATRELEASEDIR)\sl11_ser.dll             NK  SH
ENDIF

IF ODO_NOIRDA !
IF IMGNOSIR !
IF IMGNSCFIR !
   irsir.dll       $(_FLATRELEASEDIR)\irsir.dll                NK  SH
ENDIF
ENDIF
ENDIF

ENDIF

IF ODO_NOIRDA !

IF IMGNSCFIR
   nscirda.dll       $(_FLATRELEASEDIR)\nscirda.dll                NK  SH
ENDIF

ENDIF

IF ODO_NOPCMCIA !
   pcmcia.dll      $(_FLATRELEASEDIR)\pcmcia.dll                  NK  SH
ENDIF

IF CEPC_PARALLEL
;  Parallel Port Driver
   parallel.dll    $(_FLATRELEASEDIR)\parallel.dll                NK  SH
ENDIF

ENDIF
ENDIF

	rtl8139.dll      $(_FLATRELEASEDIR)\rtl8139.dll            NK  SH

FILES
;  Name            Path                                           Memory Type
;  --------------  ---------------------------------------------  -----------
IF IMG_SL11DEMO
	sl11.ini	$(_FLATRELEASEDIR)\sl11.ini		NK U
	field.bmp	$(_FLATRELEASEDIR)\field.bmp		NK U
	flower.bmp	$(_FLATRELEASEDIR)\flower.bmp		NK U
	leaf.bmp	$(_FLATRELEASEDIR)\leaf.bmp		NK U
	SFO.bmp	        $(_FLATRELEASEDIR)\SFO.bmp		NK U
ENDIF
